{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Feuil1","Feuil2","Feuil3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[[3,9,3,10],[19,9,21,9],[9,9,9,10]]}
["MESURE","LARGEUR","CATEGORIES","JANTE","PRESSION","LT","XT","LR"]
["135 R 13 TL","135","sl","3","2.2",1900,1500]
["155 R 14 TL",155,"SL","4.5","2.2",1900,1500,"C"]
["165 R 15 TL",165,"SL",5,2.2999999999999998,1900,2000,null,null,"page n° 1"]
["195 / 70 R 14 TL",195,"SL",6,"2.5",2400,2000]
["205 / 65 R 15 TL",205,"SL",6,"2.5",2400,2500,null,null,"STANDARD   (SL)","    1900 / 8.85= 214,68 (215)"]
["215/55R16 XL",215,"XL",7,"2.9",5000,2500,"E"]
["205/80 R 16 XL",205,"XL","5.5","2.8",5000,2500,"D",null,"EXTRA LOAD  (XL)","    5000 / 8,82=566,89 (567)"]
[]
[null,null,null,null,null,null,null,null,null,"page n° 2"]
[]
[null,null,null,null,null,null,null,null,null,"XT / NEWTON","1 NEWTON = 0.22480894387096"]
[]
[null,null,null,null,null,null,null,null,null,"LARGEUR BDR 160 ≤","XT = 1500  ET  NEWTON=  6670N"]
[]
[null,null,null,null,null,null,null,null,null,"LARGEUR BDR 165  ≥ 200","XT= 2000  ET  NEWTON =  8890N"]
[]
[null,null,null,null,null,null,null,null,null,"LARGEUR BDR 205+","XT=  2500  ET  NEWTON = 11120N"]
[]
[null,null,null,null,null,null,null,null,null,"Pression selon LR","C = 2,60"]
[null,null,null,null,null,null,null,null,null,null,"D = 3,40"]
[null,null,null,null,null,null,null,null,null,null,"E =  4,10"]

{"sheet":"Feuil2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}